Collection of definitions

This document contains definitions and additions to terms used in the Design specification for the post correlator integrator. This document is intended for personal review, so there is no logical sequence for the items.

Texas Instruments C40 blocks with data descriptor

This terms is for the input signal data format. I assume it defines of the operation modes of a C40 serial link. In that case the data rate probably refers to the maximum rate of the serial link.

The correlator supplies 32 input channels. If the previous assumption is correct, the entire correlator must have 32 C40 DSP's.

What is the required operation, what are the supposed operations on the input channels. Is each channel independent? i.e. is the system orthogonal for each channel or are there calculations required which involve two or more channels.